***I22-1609,***

***Ahmad Abdullah***

## DOS Box Lab02

* **mount c c:\masm615/bin:** used to mount a virtual memory for DOS Box, whereas ‘c’ is the name of virtual memory and the path is where the memory will be mounted.
* **C: :** is used to go to the C disk in the terminal.
* **masm test.asm:** Assembles the assembly language file prog.asm into an object file prog.obj.
* **link test.obj:** Links the object file prog.obj with any necessary libraries to create an executable file prog.exe.
* **ml test.asm:** Assembles the assembly language file test.asm into an object file test.obj.
* **test.exe:** Runs the executable file test.exe.

